;	[]===========================================================[]
;
;	NOTICE: THIS PROGRAM BELONGS TO AWARD SOFTWARE INTERNATIONAL(R)
;	        INC. IT IS CONSIDERED A TRADE SECRET AND IS NOT TO BE
;	        DIVULGED OR USED BY PARTIES WHO HAVE NOT RECEIVED
;	        WRITTEN AUTHORIZATION FROM THE OWNER.
;
; 	[]===========================================================[]
;

;----------------------------------------------------------------------------
;Rev	Date	 Name	Description
;----------------------------------------------------------------------------
;R28	04/28/99 PAL	Added ICS24889 Support
;R27	04/07/99 PAL	Added CY2287 Support
;R26	03/17/99 PAL	Added ICW169 Support
;R25	03/17/99 PAL	Added ICW204 Support
;R24	03/10/99 PAL	Added IMI758 Support
;R23	03/10/99 PAL	Added ICS24895 Support
;R22	03/10/99 PAL	Added ICW196 Support
;R21	03/09/99 PAL	Added PL526802 Support
;R20	02/11/99 PAL	Added ICW195 Support
;R19	02/01/99 PAL	Added ICS24879 Support
;R18	02/01/99 PAL	Added ICS24873 Support
;R17	01/30/99 PAL	Added RT52004 Support
;R16	01/29/99 PAL	Added ICW147 Support
;R15	01/12/99 PAL	Added W8319481 Support
;R14	01/08/99 PAL	Added RTM_CLOCKGEN definition for real tek 
;R13	01/06/99 PAL	Added W8319467 Support
;R12	01/04/99 PAL	Added ICS24881 Support
;R11	01/04/99 PAL	Added PL526649 Support
;R10	12/30/98 PAL	Added RT52039 Support
;R09	12/28/98 PAL	Added PL526631 Support
;R08	12/24/98 PAL	Added ICW149 Support
;R07	12/22/98 PAL	Added ICW179 Support
;R06	12/21/98 PAL	Added ICW1123 Support
;R05	12/16/98 PAL	Added ICS24877 & ICS24878 Support
;R04	12/15/98 PAL	Added ICS25010 Support
;R03	12/11/98 JDN	Added IMI_571 Support
;R02	05/14/98 PAL	Added CMA6426,6417,ICW124 ICW123 ICS5007 Support
;R01	05/08/98 PAL	Added CMA6404_Support 
;R00	03/16/98 RAY	First revision for COMMON.EQU to include
									 				
	CLKCNTL_KERNEL	=	0

;For ICWORK clock generators

ifdef	ICWORK8704_Support
	CLKCNTL_KERNEL	=	1
endif	;ICWORK8704_Support

ifdef	ICWORK8803_Support
	CLKCNTL_KERNEL	=	1
endif	;ICWORK8803_Support

ifdef	ICWORK6704_Support
	CLKCNTL_KERNEL	=	1
endif	;ICWORK6704_Support

ifdef	ICW8727_Support
	CLKCNTL_KERNEL	=	1
endif	;ICW8727_Support

ifdef	ICW8704_Support
	CLKCNTL_KERNEL	=	1
endif	;ICW8704_Support

ifdef	ICW8803_Support
	CLKCNTL_KERNEL	=	1
endif	;ICW8803_Support

ifdef	ICW6704_Support
	CLKCNTL_KERNEL	=	1
endif	;ICW6704_Support

ifdef	ICW8772_Support
	CLKCNTL_KERNEL	=	1
endif	;ICW8772_Support

ifdef	ICW6801_Support
	CLKCNTL_KERNEL	=	1
endif	;ICW6801_Support

ifdef	ICW10104_Support
	CLKCNTL_KERNEL	=	1
endif	;ICW10104_Support

ifdef	ICW11114_Support
	CLKCNTL_KERNEL	=	1
endif	;ICW11114_Support

ifdef	ICW124_Support				;R02
	CLKCNTL_KERNEL	=	1		;R02
endif	;ICW124_Support				;R02

ifdef	ICW123_Support				;R02
	CLKCNTL_KERNEL	=	1		;R02
endif	;ICW123_Support				;R02

ifdef	ICW127_Support				
	CLKCNTL_KERNEL	=	1		
endif	;ICW127_Support				

ifdef	ICW12508_Support				
	CLKCNTL_KERNEL	=	1		
endif	;ICW12508_Support				

ifdef	ICW126_Support				
	CLKCNTL_KERNEL	=	1		
endif	;ICW126_Support				

ifdef	ICW131_Support				
	CLKCNTL_KERNEL	=	1		
endif	;ICW131_Support				

ifdef	ICW13839_Support				
	CLKCNTL_KERNEL	=	1		
endif	;ICW13839_Support				

ifdef	ICW145_Support				
	CLKCNTL_KERNEL	=	1		
endif	;ICW145_Support				

ifdef	ICW148_Support				
	CLKCNTL_KERNEL	=	1		
endif	;ICW148_Support				

ifdef	ICW144_Support				
	CLKCNTL_KERNEL	=	1		
endif	;ICW144_Support				

ifdef	ICW150_Support				
	CLKCNTL_KERNEL	=	1		
endif	;ICW150_Support				

ifdef	ICW164_Support				
	CLKCNTL_KERNEL	=	1		
endif	;ICW164_Support				

ifdef	ICW160_Support				
	CLKCNTL_KERNEL	=	1		
endif	;ICW160_Support				

ifdef	ICW153_Support				
	CLKCNTL_KERNEL	=	1		
endif	;ICW153_Support				

ifdef	ICW178_Support				
	CLKCNTL_KERNEL	=	1		
endif	;ICW178_Support				

ifdef	ICW156_Support				
	CLKCNTL_KERNEL	=	1		
endif	;ICW156_Support				

ifdef	ICW167_Support				
	CLKCNTL_KERNEL	=	1		
endif	;ICW167_Support				

ifdef	ICW1123_Support				;R06
	CLKCNTL_KERNEL	=	1		
endif	;ICW1123_Support				

ifdef	ICW179_Support				;R07
	CLKCNTL_KERNEL	=	1		
endif	;ICW179_Support				

ifdef	ICW149_Support				;R08
	CLKCNTL_KERNEL	=	1		
endif	;ICW149_Support				

ifdef	ICW147_Support				;R16
	CLKCNTL_KERNEL	=	1		
endif	;ICW147_Support				

ifdef	ICW195_Support				;R20
	CLKCNTL_KERNEL	=	1
endif	;ICW195_Support

ifdef	ICW196_Support				;R22
	CLKCNTL_KERNEL	=	1
endif	;ICW196_Support

ifdef	ICW204_Support				;R25
	CLKCNTL_KERNEL	=	1
endif	;ICW204_Support

ifdef	ICW169_Support				;R26
	CLKCNTL_KERNEL	=	1
endif	;ICW169_Support

ifdef	KS8448_Support
	CLKCNTL_KERNEL	=	1
endif	;KS8448_Support

;for Cypress clock generators	
ifdef	CY2275_Support
	CLKCNTL_KERNEL	=	1
endif;	CY2275_Support

ifdef	CY2283_Support
	CLKCNTL_KERNEL	=	1
endif;	CY2283_Support

ifdef	CY2318NZ_Support
	CLKCNTL_KERNEL	=	1
endif;	CY2318NZ_Support

ifdef	CY2277_Support
	CLKCNTL_KERNEL	=	1
endif;	CY2277_Support

ifdef	CY2287_Support			;R27
	CLKCNTL_KERNEL	=	1
endif;	CY2287_Support

;For IMI clock generators

ifdef	IMI743_Support		 
	CLKCNTL_KERNEL	=	1
endif	;IMI743_Support		 

ifdef	IMI643_Support
	CLKCNTL_KERNEL	=	1
endif	;IMI643_Support

ifdef	IMI543_Support
	CLKCNTL_KERNEL	=	1
endif	;IMI543_Support

ifdef	IMI671_Support
	CLKCNTL_KERNEL	=	1
endif	;IMI671_Support

ifdef	IMI571_Support				;R03 
	CLKCNTL_KERNEL	=	1		;R03
endif	;IMI571_Support				;R03
						
ifdef	IMI584_Support
	CLKCNTL_KERNEL	=	1
endif	;IMI584_Support

ifdef	IMI745_Support
	CLKCNTL_KERNEL	=	1
endif	;IMI745_Support

ifdef	IMI758_Support				;R24
	CLKCNTL_KERNEL	=	1		
endif	;IMI758_Support				

;For ICS clock generators
ifdef	ICS4833_Support
	CLKCNTL_KERNEL	=	1
endif	;ICS4833_Support

ifdef	ICS4826_Support
	CLKCNTL_KERNEL	=	1
endif	;ICS4826_Support

ifdef	ICS4837_Support
	CLKCNTL_KERNEL	=	1
endif	;ICS4837_Support

ifdef	ICS9148_Support
	CLKCNTL_KERNEL	=	1
endif	;ICS9148_Support

ifdef	ICS9150_Support
	CLKCNTL_KERNEL	=	1
endif	;ICS9150_Support

ifdef	ICS7901_Support
	CLKCNTL_KERNEL	=	1
endif;	ICS7901_Support

ifdef	ICS4847_Support
	CLKCNTL_KERNEL	=	1
endif	;ICS4847_Support

ifdef	ICS4804_Support
	CLKCNTL_KERNEL	=	1
endif	;ICS4804_Support

ifdef	ICS5004_Support
	CLKCNTL_KERNEL	=	1
endif	;ICS5004_Support

ifdef	ICS4836_Support
	CLKCNTL_KERNEL	=	1
endif	;ICS4836_Support

ifdef	ICS4837_Support
	CLKCNTL_KERNEL	=	1
endif	;ICS4837_Support

ifdef	ICS5007_Support				;R02
	CLKCNTL_KERNEL	=	1		;R02
endif	;ICS5007_Support			;R02

ifdef	ICS4832_Support				
	CLKCNTL_KERNEL	=	1		
endif	;ICS4832_Support			

ifdef	ICS5008_Support				
	CLKCNTL_KERNEL	=	1		
endif	;ICS5008_Support			

ifdef	ICS4812_Support				
	CLKCNTL_KERNEL	=	1		
endif	;ICS4812_Support			

ifdef	ICS4858_Support				
	CLKCNTL_KERNEL	=	1		
endif	;ICS4858_Support			

ifdef	ICS4853_Support				
	CLKCNTL_KERNEL	=	1		
endif	;ICS4853_Support			

ifdef	ICS25008_Support				
	CLKCNTL_KERNEL	=	1		
endif	;ICS25008_Support			

ifdef	ICS24839_Support				
	CLKCNTL_KERNEL	=	1		
endif	;ICS24839_Support			

ifdef	ICS24859_Support				
	CLKCNTL_KERNEL	=	1		
endif	;ICS24859_Support			

ifdef	ICS24867_Support				
	CLKCNTL_KERNEL	=	1		
endif	;ICS24867_Support			

ifdef	ICS4875_Support				
	CLKCNTL_KERNEL	=	1		
endif	;ICS4875_Support			

ifdef	ICS24868_Support				
	CLKCNTL_KERNEL	=	1		
endif	;ICS24868_Support			

ifdef	ICS25010_Support			;R04
	CLKCNTL_KERNEL	=	1		
endif	;ICS25010_Support			

ifdef	ICS24877_Support			;R05
	CLKCNTL_KERNEL	=	1		
endif	;ICS24877_Support			

ifdef	ICS24878_Support			;R05
	CLKCNTL_KERNEL	=	1		
endif	;ICS24878_Support			

ifdef	ICS24881_Support			;R12
	CLKCNTL_KERNEL	=	1		
endif	;ICS24881_Support			

ifdef	ICS24873_Support			;R18
	CLKCNTL_KERNEL	=	1		
endif	;ICS24873_Support			

ifdef	ICS24879_Support			;R19
	CLKCNTL_KERNEL	=	1		
endif	;ICS24879_Support			

ifdef	ICS24895_Support			;R23
	CLKCNTL_KERNEL	=	1		
endif	;ICS24895_Support			

ifdef	ICS24889_Support			;R28
	CLKCNTL_KERNEL	=	1		
endif	;ICS24889_Support			

;for Phaselink clock generators
ifdef	PL526502_Support
	CLKCNTL_KERNEL	=	1
endif;	PL526502_Support

ifdef	PL526601_Support
	CLKCNTL_KERNEL	=	1
endif;	PL526601_Support

ifdef	PL526623_Support
	CLKCNTL_KERNEL	=	1
endif;	PL526623_Support

ifdef	PL526301_Support
	CLKCNTL_KERNEL	=	1
endif;	PL526301_Support

ifdef	PL526618_Support
	CLKCNTL_KERNEL	=	1
endif;	PL526618_Support

ifdef	PL526609_Support
	CLKCNTL_KERNEL	=	1
endif;	PL526609_Support

ifdef	PL526619_Support
	CLKCNTL_KERNEL	=	1
endif;	PL526619_Support

ifdef	PL526425_Support
	CLKCNTL_KERNEL	=	1
endif;	PL526425_Support

ifdef	PL526629_Support
	CLKCNTL_KERNEL	=	1
endif;	PL526629_Support

ifdef	PL526628_Support
	CLKCNTL_KERNEL	=	1
endif;	PL526628_Support

ifdef	PL526638_Support
	CLKCNTL_KERNEL	=	1
endif;	PL526638_Support

ifdef	PL526639_Support
	CLKCNTL_KERNEL	=	1
endif;	PL526639_Support

ifdef	PL526804_Support
	CLKCNTL_KERNEL	=	1
endif;	PL526804_Support

ifdef	PL526631_Support			;R09
	CLKCNTL_KERNEL	=	1
endif;	PL526631_Support

ifdef	PL526649_Support			;R11
	CLKCNTL_KERNEL	=	1
endif;	PL526649_Support

ifdef	PL526802_Support			;R21
	CLKCNTL_KERNEL	=	1
endif;	PL526802_Support

;for Winbond clock generators
ifdef	W8319301_Support
	CLKCNTL_KERNEL	=	1
endif;	W8319301_Support

ifdef	W8319302_Support
	CLKCNTL_KERNEL	=	1
endif;	W8319302_Support

ifdef	W8319417_Support
	CLKCNTL_KERNEL	=	1
endif;	W8319417_Support

ifdef	W8319439_Support
	CLKCNTL_KERNEL	=	1
endif;	W8319439_Support

ifdef	W8319437_Support
	CLKCNTL_KERNEL	=	1
endif;	W8319437_Support

ifdef	W8319614_Support
	CLKCNTL_KERNEL	=	1
endif;	W8319614_Support

ifdef	W8319458_Support
	CLKCNTL_KERNEL	=	1
endif;	W8319458_Support

ifdef	W8319459_Support
	CLKCNTL_KERNEL	=	1
endif;	W8319459_Support

ifdef	W8319467_Support			;R13
	CLKCNTL_KERNEL	=	1
endif;	W8319467_Support

ifdef	W8319481_Support			;R15
	CLKCNTL_KERNEL	=	1
endif;	W8319481_Support

;for C-Media clock generators			;R01
ifdef	CMA6404_Support				;R01
	CLKCNTL_KERNEL	=	1		;R01
endif;	CMA6404_Support				;R01

ifdef	CMA6417_Support				;R02
	CLKCNTL_KERNEL	=	1		;R02
endif;	CMA6417_Support				;R02

ifdef	CMA6426_Support				;R02
	CLKCNTL_KERNEL	=	1		;R02
endif;	CMA6426_Support				;R02

;for Real Tek clock generators			

ifdef	RT52039_Support				;R10
	CLKCNTL_KERNEL	=	1		;R10
ifdef	RT52039_Freq_Cntl
	RTM_CLOCKGEN 	equ	1		;R14
endif;	RT52039_Freq_Cntl
endif;	RT52039_Support				;R10

ifdef	RT52004_Support				;R17
	CLKCNTL_KERNEL	=	1		;R17
ifdef	RT52004_Freq_Cntl			;R17
	RTM_CLOCKGEN 	equ	1		;R17
endif;	RT52004_Freq_Cntl			;R17
endif;	RT52004_Support				;R17

