Failed experiments:
 
  - Direct entry into RING 3 via VCPI (PRO3VCPI.ASM)
       - Not going to work. VCPI servers assume you're entering into ring 0.
       - Entering with a ring 3 address directly is not possible because of VCPI's ring 0 selectors.

