PCE Messages
==============================================================================

Messages are used to control the emulator. They can be sent using the "m"
command in the monitor, for example

-m emu.disk.eject 0

will eject the first floppy disk. Message prefixes can be omitted, as long
as the message name is unambiguous (except where noted). The following
commands are equivalent:

-m emu.disk.eject 0
-m disk.eject 0
-m eject 0

A message has at most one parameter. If the parameter contains spaces, it
must be enclosed in double quotes in the monitor, like this:

-m term.screenshot "my screenshot.ppm"


PCE/ibmpc Messages
==============================================================================

emu.exit
	Terminate the emulator immediately.

emu.stop
	Fall back to the monitor.

emu.pause "0" | "1"
	Resume or pause the emulator.

emu.pause.toggle
	Resume or pause the emulator.

emu.reset
	Reset the emulated machine.

emu.config.save <filename>
	Save the current configuration to <filename>.

emu.cpu.model <model>
	Set the emulated CPU model. Valid models are "8086", "8088",
	"80186" and "80188".

emu.cpu.speed <factor>
	Set the emulated CPU clock frequency to a multiple of 4.77 MHz.

emu.cpu.speed.step <adjustment>
	Add <adjustment> to the CPU clock frequency multiplier.

emu.disk.boot <bootdrive>
	Set the boot drive.

emu.disk.commit (<drive> [":" <drive> ...]) | "all"
	Commit changes to drives that have copy-on-write enabled.

emu.disk.eject <drive> [":" <drive> ...]
	Eject the disk in drive <drive>.

emu.disk.insert <drive>:<fname>
	Insert a new disk. <drive> is a drive number as specified
	in the config file. The disk image type is "auto". If a disk
	is already inserted in <drive> it is ejected first.

emu.parport.driver <port>":"<driver>
	Attach a parallel port to a new character driver. The driver
	string has the same format as in the config file.

emu.parport.file <port>":"<filename>
	This is equivalent to
	emu.parport.driver <port>:stdio:file=<filename>.

emu.serport.driver <port>":"<driver>
	Attach a serial port to a new character driver. The driver
	string has the same format as in the config file.

emu.serport.file <port>":"<filename>
	This is equivalent to
	emu.serport.driver <port>:stdio:file=<filename>.

emu.tape.append
	Move the read or write position to the end of the cassette file.

emu.tape.file <filename>
	Set a new cassette file. If the file name ends with ".pcm" or
	".raw" then PCM mode is automatically enabled. If the file
	name ends with ".cas" then binary mode is automatically
	disabled. In all other cases the current PCM mode is not
	changed.

emu.tape.filter "0" | "1"
	Disable or enable PCM output filtering.

emu.tape.load [<position> | "end"]
	Switch to load mode. If <position> is given, move the load
	position to <position>. If "end" is specified, move the load
	position to the end of the cassette file.

emu.tape.pcm "0" | "1"
	Disable or enable PCM mode.

emu.tape.rewind
	Move the read or write position to the beginning of the cassette
	file.

emu.tape.save [<position> | "end"]
	Switch to save mode. If <position> is given, move the save
	position to <position>. If "end" is specified, move the save
	position to the end of the cassette file.

emu.tape.state
	Print the cassette state. Prints the current mode (load/save)
	and the current position.

emu.video.blink <blink-rate>
	Set the cursor blink rate. The number specified is the number
	of screen refreshes for which the cursor is visible/invisible.

emu.video.redraw ["0" | "1"]
	Force a redraw of the screen. If the parameter is "1", redraw
	immediately, otherwise schedule a forced redraw at the next
	vertical retrace.


PCE/macplus Messages
==============================================================================

emu.cpu.model <model>
	Set the emulated CPU model. Valid models are "68000" and "68010".

emu.cpu.speed <speed>
	Set the emulated CPU clock frequency to a multiple of 7.8336MHz.

emu.cpu.speed.step <step>
	Add <step> to the CPU clock frequency multiplier.

emu.disk.commit (<drive> [":" <drive> ...]) | "all"
	Commit changes to drives that have copy-on-write enabled.

emu.disk.eject <drive> [":" <drive> ...]
	Eject the disk in drive <drive>.

emu.disk.insert <drive>:<fname>
	Insert a new disk. <drive> is a drive number as specified
	in the config file. The disk image type is "auto". If a disk
	is already inserted in <drive> it is ejected first.

emu.disk.ro <drive>
	Set the read-only flag for the disk in drive <drive>.

emu.disk.rw <drive>
	Clear the read-only flag for the disk in drive <drive>.

emu.exit
	Terminate the emulator immediately.

emu.fdc.accurate "0" | "1"
	Disable or enable the FDC accurate mode.

emu.pause "0" | "1"
	Pause or resume the emulation.

emu.pause.toggle
	Pause or resume the emulation.

emu.reset
	Reset the emulated machine.

emu.serport.driver <port>":"<driver>
	Attach a serial port to a new character driver. The driver
	string has the same format as in the config file.

emu.serport.file <port>":"<filename>
	This is equivalent to
	emu.serport.driver <port>:stdio:file=<filename>.

emu.stop
	Fall back to the monitor.

emu.video.brightness <brightness>
	Set the video brightness in the range of 0 - 1000.

mac.insert [<drive>]
	Simulate re-inserting a disk that has been dragged to the trash.


Terminal messages
==============================================================================

Terminal messages may not be abbreviated.

term.fullscreen "0" | "1"
	Leave or enter fullscreen mode.

term.fullscreen.toggle
	Toggle fullscreen mode.

term.grab
	Grab the mouse.

term.release
	Release the mouse.

term.screenshot [<filename>]
	Write a screen shot to <filename> in PNM format.

term.title <title>
	Set the terminal window title.
